For sftp, when loss is greater, the time consumption is greater. 15% is little smaller than 10%, should be some good luck.

For sftp, when delay is higher, the time consumption is much greater. With 400ms delay, the time is almost to 1min.

For gftp, when window size is higher, the time consumption is significantly smaller, in theory should be halved by each, which is expected in graph.

In all, the data is as expected.